Çekirdek Mesajları

Next: Linux Dosya Sistemi Yapısı Up: Linux Sistem Yönetimi Previous: /etc/rc.d/* Dosyaları

# Çekirdek Mesajları

Çekirdek, hafızaya yüklenip çalıştırıldıktan sonra kendisi ve sistemdeki donanım hakkındaki her türlü bilgiyi ekrana yazar. Her türlü bilginin içine hata mesajları da girer. Çekirdeğin hata verip vermemesi açılış anında ekrana bakmakla anlaşılabilir. Bu nedenle sistem açılırken gözünüzü monitörden ayırmamalısınız. Aşağıda bir çekirdeğin açılış kaydı yeralıyor :

    Console: colour EGA+ 80x25, 1 virtual console (max 63)
    bios32_init : BIOS32 Service Directory structure at 0x000faf10
    bios32_init : BIOS32 Service Directory entry at 0xfb390
    pcibios_init : PCI BIOS revision 2.10 entry at 0xfb3c0
    Calibrating delay loop.. ok - 30.22 BogoMips
    Serial driver version 4.11 with no serial options enabled
    tty00 at 0x03f8 (irq = 4) is a 16550A
    tty01 at 0x02f8 (irq = 3) is a 16550A
    lp1 at 0x0378, using polling driver
    ftape: allocated 3 buffers aligned at: 00210000
    hda: QUANTUM ELS170A, 162MB w/32KB Cache, CHS=1011/15/22, MaxMult=8
    ide0: primary interface on irq 14
    Floppy drive(s): fd0 is 1.44M
    FDC 0 is a post-1991 82077
    lance.c: PCI bios is present, checking for devices...
    Memory: 6612k/8192k available (760k kernel code, 384k reserved, 436k data)
    This processor honours the WP bit even when in supervisor  mode. Good.
    Swansea University Computer Society NET3.019
    Swansea University Computer Society TCP/IP for NET3.019
    IP Protocols: ICMP, UDP, TCP
    PPP: version 0.2.7 (4 channels) NEW_TTY_DRIVERS OPTIMIZE_FLAGS
    TCP compression code copyright 1989 Regents of the University of California
    PPP line discipline registered.
    SLIP: version 0.8.3-NET3.019-NEWTTY (4 channels) (6 bit encapsulation enabled)
    CSLIP: code copyright 1989 Regents of the University of California
    eth0: D-Link DE-600 pocket adapter: at I/O 0x378.
    Checking 386/387 coupling... Ok, fpu using exception 16 error reporting.
    Checking 'hlt' instruction... Ok.
    Linux version 1.2.13 (root@bigkitty) (gcc version 2.7.0)
    Partition check:
      hda: multiple mode turned off
      hda: hda1 hda2
    VFS: Mounted root (ext2 filesystem) readonly.
    Adding Swap: 8188k swap-space

Yukarıdaki mesajda takas alanı belirlenmesi, sabit diskin tanınması, disketin tanınması, aygıt sürücülerinin, ethernet kartını tanıması ve ekranın özelliklerinin yazılması gibi bilgiler vardır. Bu bilgilere sistem açıldıktan sonra `/var/adm/messages` dosyasıından da erişilebilir.